Annex No. 1
 
 
PROPOSAL 
 
Under the EU European Agricultural Fund for Rural Development (EAFRD) Measure 4. 'Investments in tangible assets' Sub-measure 4.2 'Support for investments in processing'
 
	1. Client:
	AS "Ķekava Foods” 

	2. Taxpayer registration number:
	LV 50003007411 

	3. Client address:  
	Ziemeļu iela 55, Ķekava, Ķekavas nov., LV-2123

	4. Ordered item and quantity:
	Sausage linking and hanging system – 1 unit

	5. Delivery location:
	AS "Ķekava Foods”, Ziemeļu iela 55, Ķekava, Ķekavas nov., LV-2123

	6. Delivery date:
	30.08.2026. 

	7. Offer validity period:
	till 30.08.2026. 

	8. Technical specification:  
	 


 
	Requirements
	Supplier parameters

	Sausage linking and hanging system – 1 unit
	Manufacturer:
Brand:
Model:

	1
	Minimum portioning speed, portions/min with natural casing – 5800
	

	2
	Minimum portioning speed, portion/min with artificial and collagen casing - 2000
	

	3
	Must have semi-automated casing change function
	

	4
	Casing caliber, range from–to, mm – 15–40
	

	5
	Portion weight range, from–to, g – 20–200
	

	6
	Minimum product length, mm – ≤ 40
	

	7
	Maximum product length, mm – ≥ 200
	

	8
	Automatic product hanging system
	

	9
	Hanging line length, not less than, mm – 2300
	

	10
	Casing end sensor
	

	11
	Calibre setting with digital display
	

	12
	X40 socket conectivity and compatability
	

	13
	Korpuss no nerūsējoša tērauda.
	

	14
	Minimum moisture protection class - IP65
	

	15
	Documentation - must include the equipment's operating instructions in Latvian, a spare parts catalog, an electrical diagram, and a pneumatic diagram.
	

	Sausage filling machine – 2 pc.
	Manufacturer:
Brand:
Model:

	1
	Filling capacity, not less than, kg/h - 5800
	

	2
	Portioning speed,  not less than portions/min - 1200
	

	3
	Expected product weight limits, from-to, g - <=5 - >=200000
	

	4
	Portioning accuracy per portion, not less than ±1%
	

	5
	Filling pressure not less than 70 bar
	

	6
	With servo driven screw down version rotor and vane system for meat mass pumping
	

	7
	Vacuum function adjustable 0-100%, with vacuum pump not less than 40 m3/h
	

	8
	With pressure sensor in meat pump outlet
	

	9
	The volume of the filler tank, not less than, liters - 240, dividable
	

	10
	Stainless steel body
	

	11
	Lift for 200l trolleys with automatic trolley locking
	

	12
	Machine width no more than 1750 mm
	

	13
	Equipment length no more than 2500 mm
	

	14
	The height of the machine, including the raised trolley, does not exceed 2970 mm
	

	15
	The filler is designed for mass with a temperature from +2°C to +40°C
	

	16
	Metal detectable design of all non-metallic machine components in food contact areas
	

	17
	Compatibility with HV 60-6  Serial No. 2853 and 2426
	

	18
	X40 socket conectivity 
	

	19
	The filler is designed to work with homogeneous mass and mass with lumps (maximum lump sizes - 10x15x10 mm)
	

	20
	Minimum moisture protection class - IP65
	

	21
	Documentation - must include the equipment's operating instructions in Latvian, a spare parts catalog, an electrical diagram, and a pneumatic diagram.
	



Warranty Period: ______________
Defect Rectification: ____ hours.
Spare Parts Availability: ____ hours.


Supplier Information 
Company Name:
Registration No.: 
Equipment Brand and Model: 
Estimated Contract Execution Period: 
Valid Until:
Price (EUR, excluding VAT):
Proposal Date:
Prepared by:
Position: 
Email:
Phone: 





Annex No. 2 
 
AS "Ķekava Foods”  
/Customer Name/  
 
Declaration of Independent Proposal

Hereby, providing complete and truthful information,
____________________________________________________________________
[Supplier’s Name, Registration No.]
(hereinafter – Suppliert) with regard to the specific procurement procedure declares that:
1. The Supplier has reviewed and agrees to the content of this declaration.
2. The Supplier acknowledges its obligation to provide complete, comprehensive, and truthful information in this declaration.
3. The Supplier’s procurement proposal has been signed by the Supplier’s authorized person(s).
4. The Supplier confirms that the proposal has been submitted independently of competitors and without consultations, agreements, or arrangements. The Supplier has not communicated with any competitor regarding:
4.1. Prices;
4.2. Price calculation methods, factors (conditions), or formulas;
4.3. Intentions or decisions to participate or not participate in the procurement (to submit or not submit a proposal);
4.4. Submission of a proposal that does not meet the procurement requirements;
4.5. Quality, quantity, specifications, execution, delivery, or other conditions that must be addressed independently of competitors for the products or services covered by this procurement.
5. The Supplier has not knowingly, directly or indirectly, disclosed and will not disclose the terms of the proposal to any competitor before the official proposal opening date and time or the award of contract rights.
6. The Supplier acknowledges that the Competition Law establishes liability for prohibited agreements, providing for a fine of up to 10% of the offender’s net turnover from the last financial year, and the Supplier may be excluded from participating in the procurement procedure.

Date:
Signature: 


