Annex No. 2

TECHNICAL SPECIFICATION

PURCHASE OF AUTOMATIC TILTING CYLINDRICAL BOILING PAN WITH MIXER 
place, date
The following table:
	Parameter
	Requirement

	THE PARTICIPANT shall provide information or proof against each requirement.
	

	Quantity
	2 pcs. – Industrial automatic tilting boiling pan with integrated mixer and PLC control.

	Brand, model offered
	Brand name (for identification purposes) and model name (for identification purposes).

	Purpose
	Large capacity industrial cooking (boiling, mixing) for mass catering. The unit must feature an automatic mixer and a tilting system designed to unload food into trolleys while maintaining a constant outlet height.


	Capacity
	• Tank Capacity: 280 – 320 litres.


	Construction
	• Material: Double-walled vessel made of stainless steel (AISI-304/316).


• Design: Cylindrical structure with a high discharge point suitable for 200L trolleys.


• Hygiene: Certified IPX5 protection or equivalent.

	Heating System
	• Type: Indirect Electric heating.


• Technology: Heated by armoured heating elements immersed in the double jacket water/oil bath.

	Mixer System
	• Type: Integrated automatic mixer with adjustable speed.


• Blades: Mixing blades must be customizable and easy to remove for cleaning.

	Tilting Mechanism
	• Type: Motorised automatic tilting.

• Functionality: The pouring lip/outlet must remain at the same height during the tilting process to facilitate safe unloading into trolleys.


	Control System
	• Interface: Advanced PLC monitor with a Touch Screen.


• Functions: Automation of cooking parameters, recipe management, mixer control, and tilting control.

	Power & Voltage
	• Total Electric Power: 45 kW – 50 kW.


• Voltage: 400V / 3 ph / 50 Hz.

	Dimensions
	• Length: 1500 – 1600 mm.


• Depth: 1550 – 1650 mm.


• Height: 1200 – 1300 mm.


	Mandatory Accessories (Included)
	The supplier is responsible for providing a fully functional unit with the following specific accessories included:


• Shower kit / Flexible hose for cleaning.

• Automatic device for filling the tank with water.

• Electronic water meter / Automatic water charge control system.

• Filter/Strainer for the pouring lip.

	Documentation
	To be supplied in Latvian or English: user manual, electric diagram, maintenance instructions, CE Declaration of Conformity.

	Compliance
	Equipment must comply with EU Machinery Directive 2006/42/EC and food contact materials legislation. CE marking mandatory.

	Guarantee
	Minimum 24 months full manufacturer or supplier warranty.


Name, surname, position
signature
