Annex No. 2

TECHNICAL SPECIFICATION

PURCHASE OF REFRIGERATED FISH STORAGE CABINET
place, date
The following table:
	Parameter
	Requirement

	THE PARTICIPANT shall provide information or proof against each requirement.
	

	Quantity
	5 pcs. – Vertical refrigerated cabinet specifically designed for fresh fish storage.

	Brand, model offered
	Brand name (for identification purposes) and model name (for identification purposes).

	Purpose
	Storage of fresh fish and seafood at specific negative/positive temperatures to prevent spoilage and dehydration.

	Temperature Range
	• Working Temperature: Adjustable range covering -4°C to +4°C to ensure optimal preservation of fresh fish.

	Capacity & Storage
	• Storage Levels: Designed to hold at least 7 levels of fish containers.

• Container Size: Compatible with 600x400 mm containers/bins.

• Included Containers: The unit must be supplied with a full set of 7 x specialty fish containers (stainless steel or food-grade plastic with perforated bottoms for drainage).

	Construction
	• Material: Interior and exterior made of high-quality Stainless Steel to resist corrosion from salts and fluids.

• Insulation: High-density polyurethane, thickness 50 mm or higher

• Drain: Integrated drainage system at the bottom for the evacuation of waste liquids/ice melt, crucial for fish hygiene.

• Protection: IPX5 water protection rating or equivalent.

	Cooling System
	• Type: Top-mounted refrigeration unit.

• Refrigerant: Environmentally friendly hydrocarbon R290 (ECO mode capable).

• Climate Class: 4 (up to 30°C ambient).

• Defrost: Automatic electric defrosting.

	Control System
	• Interface: Electronic control with a capacitive touch screen minimum 3 inches).

• Functions: Temperature display, HACCP alarm history (optional but preferred), ECO mode.

	Dimensions
	• Width: 640 mm – 760 mm.

• Depth: 700 mm – 820 mm.

• Height: 1980 mm – 2020 mm.

	Door
	• Type: Solid stainless steel door.

• Features: Self-closing mechanism, stay-open feature at 90°, ergonomic full-length handle.

	Complete Functional Set (Mandatory)
	The supplier is responsible for providing a fully functional unit ready for immediate use. The set must include:

• 1 x Refrigerated Cabinet Unit

• 7 x Fish Storage Containers (600x400 mm)

• Adjustable stainless steel legs (130-200 mm)

• Power cable and plug

	Documentation
	To be supplied in Latvian or English: user manual, electric diagram, maintenance instructions, CE Declaration of Conformity.

	Compliance
	Equipment must comply with EU Machinery Directive 2006/42/EC, Low Voltage Directive, and food contact materials legislation. CE marking mandatory.

	Guarantee
	Minimum 24 months full manufacturer or supplier warranty.


Name, surname, position
signature
