
Annex No. 2
Technical Specification
Purchase of Industrial Complete Cleaning Stations with Hose Reel (Satellite System)

	Parameter
	Requirement

	THE PARTICIPANT shall provide information or proof against each requirement.
	

	Quantity
	16 pcs. – Complete Cleaning Stations with Integrated Hose Reel (Satellite Stations).

	Purpose
	To function as a basic, non-mobile element of a central cleaning system. The station must provide all elements necessary for preliminary rinsing, foaming, disinfection, and final rinsing processes.

	1. System Type and Construction
	

	* System Type
	Designed as a satellite station (e.g., SR 25-1 class or equivalent) for connection to a central high-pressure water main.

	* Material
	Constructed from high-grade stainless steel (AISI 304 or equivalent) for exceptional durability, reliability, and chemical resistance.

	* Design
	Robust, hygienic design with convenience of use being paramount.

	2. Operational Performance
	

	* Water Input Pressure
	Designed to operate with a central water supply pressure of 20 bar – 30 bar.

	* Water Flow Rate
	Working flow rate: 12 L/min – 18 L/min (suitable for single-user intensive cleaning).

	* Cleaning Stages
	Must facilitate sequential stages: preliminary rinsing (with high-pressure water), foam application, intermediate rinsing, disinfectant application, and final rinsing.

	3. Mandatory Components (Complete Kit)
	

	* Satellite Station
	The core wall-mounted control/mixing unit (e.g., SR 25-1).

	* Hose Reel
	Integrated stainless steel hose reel (manual or automatic).

	* Hose
	Supplied with a minimum of 20 metres – 25 metres of high-pressure hose (double metal braided or equivalent industrial standard).

	* Lances/Nozzles
	A complete set of lances for three separate applications: washing/rinsing, foam application, and disinfection.

	* Chemical Integration
	Container hanger/basket for chemical agents (detergents/disinfectants).

	* Accessories
	Includes lance hanger, butterfly valves, quick couplings, and necessary connection hoses.

	Complete Functional Set (Mandatory)
	The Supplier must ensure that all components and preparation of the machine are completed for full operation. If data is lacking, the supplier must contact the procurement department. The offer must explicitly include: the satellite station, the hose reel, the high-pressure hose, and the complete set of lances/nozzles, fully installed and ready for connection to the central system.

	Documentation
	To be supplied in Latvian or English: user manual, electric diagram, maintenance instructions, and CE Declaration of Conformity.

	Guarantee
	Minimum 24 months full manufacturer or supplier warranty.



