
Annex No. 2
TECHNICAL SPECIFICATION
PURCHASE OF WHEY PROCESSING EQUIPMENT


________________________
place, date

	Parameter

	Requirement

	THE PARTICIPANT shall provide information or proof against each requirement.


	Quantity
	1 pc. reverse osmosis unit with integrated polisher
1 pc. whey heating device
1 pc. whey vibration separator
1 pc. whey separation equipment integration
1 pc. whey concentrate cooling unit
1 pc. mechanical assembly materials for connecting units and
           storage
1 pc. MCC cabinets and cables
1 pc. Equipment and line automation
1 pc. Monitoring mechanical and electrical installation
	

	Quality
	Meets EU food industry equipment requirements and standards (in accordance with EU Regulation (EC) No. 1935/2004 on materials coming into contact with food)
	

	Productivity line
	RO unit with integrated polisher
30 m³/h, whey up to 30% dry matter
20 m³/h, skimmed milk up to 35% dry matter content
30 m³/h, whey vibration separator and whey heating
	

	RO/PO unit
	CIP dosing machine
Dosing device for pH reduction
	

	Whey heating
	Whey: Heating: 72°C–75°C, Cooling 2–6°C
Max. 2 K temperature difference between whey and hot water circulation
	

	Retentate cooling
	Whey and skimmed milk Cooling 2°C - 6°C, capacity 4,000 l/h - 5,500 l/h
	

	Engines
	Energy-reduced IE4 class motors, if applicable
	

	Connection with:
	Storage of raw whey
Whey storage
Whey/milk concentrate storage
Polisher water storage
Heat oscillation system
	

	Mechanical assembly material

	Valves (, pumps, measurement and control technology)
Pipes and holders
	

	Materials used
	AISI316 stainless steel

	

	Documentation
	in Latvian or English (declarations of conformity, equipment passports, user manuals, maintenance, use and repair instructions, electrical and pneumatic diagrams (if applicable).
	

	Labeling
	CE

	

	Compliance with European Mechanical Engineering Standards
directives
	Complies with EU directive
(the declaration of conformity must be submitted to the Customer together with other documents specified in the specification, by signing the acceptance-handover protocol)
	

	Security

	Meets EU industry standard requirements
	




________________________________
Name, surname, position
____________________
signature


