Delivery of components for the Mobile Robot Cloud Edge System - delivery of an autonomous and fully programmable humanoid robot
Procurement  ID no.K/2025/281125/13
“Nākamās paaudzes mikroražotnes”, Nr.5.1.1.2.i.0/4/24/A/CFLA/003
	1. Finansējuma saņēmējs - Pasūtītājs/Beneficiary of financing - Contracting Authority

	Nosaukums/Name
	SIA Aspired

	Vienotais reģ. Nr./
Registration number
	41203045860

	Juridiskā adrese/
Legal address
	Ganību iela 99, Ventspils, Latvija, LV-3601

	Kontaktpersona/
Contact person (contact point)
	Toms Vācietis, tālruņa numurs: +371 29476782, e-pasta adrese: toms.vacietis@aspired.lv



	2. Informācija par priekšmetu/Subject of procurement

	Iepirkuma nosaukums/
Title of procurement
	Komponenšu piegāde Mobilo robotu mākoņmalas sistēmai - autonoma programmējama humanoīda robota piegāde/
Delivery of components for the Mobile Robot Cloud Edge System - delivery of an autonomous and fully programmable humanoid robot

	Iepirkuma identifikācijas numurs/
Procurement identification number
	K/2025/281125/13

	Iepirkuma priekšmets/
Description of the subject of procurement
	Viena autonoma programmējama humanoīda robota piegāde industriālu uzdevumu risinājumiem  (turpmāk - Piegādes)/
Delivery of one autonomous and fully programmable humanoid robot (hereinafter - Deliveries)

	Piegādes laiks
	Ne vēlāk kā 10 (desmit) kalendāra nedēļu laikā no līguma noslēgšanas brīža./
No later than 10 (ten) calendar weeks from the date of conclusion of the contract.



	3. Piedāvājuma iesniegšana/Submission of offer

	3.1.
	Procurement proposals, together with duly completed technical and financial offer forms as set out in this document, shall be submitted electronically to info@aspired.lv

	3.2.
	The tender proposals will be opened in the order in which they were submitted. If two or more bids offer the same price, the contract will be awarded to the bid submitted first.

	3.3.
	The tenderer has the right to amend or withdraw its procurement proposal until the deadline for submitting bids.

	3.4.
	The tenderer shall cover all expenses related to the preparation and submission of the procurement proposal. The contracting authority is not responsible for, does not cover or compensate for these expenses, regardless of the course and outcome of the procurement.



	4. Tehniskās specifikācijas/Technical specifications of Subject of Procurement


	
#
	Characteristic
	Requirement
	Technical Proposal
(fill in “yes” or specific technical parameter if applicable)

	1
	Key dimensions
	Total height not less than 1500mm
	

	2
	Degrees of Freedom (DOF) of each leg
	Not less than 7
	

	3
	Degrees of Freedom (DOF) of each arm
	Not less than 5
	

	4
	Type of arms
	Dexterous arms suitable for industrial manipulation tasks: (1) force controlled three-fingered dexterous hand (left) (2) multi-joint five-fingered dexterous hand (right)
	

	5
	Number of arms
	2 arms
	

	6
	Weight that can be lifted with one hand in movement
	Not less than 5 kg
	

	7
	Total weight
	Total mass not more than 100 kg
	

	8
	Computing power
	Integrated onboard computing with performance equivalent to a modern multi-core processor suitable for 
· real-time robot control,
· sensor processing,
· and continuous background execution of third-party applications
	

	9
	External compute compatibility
	The system must allow integration of an additional external compute module
	

	10
	Battery
	Battery capacity not less than 800 Wh or providing at least 2 hours of operation
	

	11
	Exchangable batteries included
	Yes, 3 interchangeable (hot-swappable) humanoid robot batteries included
	

	12
	Dock station included
	Yes, supplier must specify functionality
	

	13
	Sensor
	3D lidar with a minimum of 16 channels, depth camera
	

	14
	Included in the package
	Protective lift bracket (crane), remote control, fast charger
	

	15
	Compatibility
	4G, Wi-Fi 6, Bluetooth 5.2 (equivalent or newer)
	

	16
	Communication & I/O interfaces
	Must include at least: 
· ethernet port, 
· USB-A or USB-C port, 
· industrial communication bus
	

	17
	End-effector integration capability
	Both arms must support modular end-effector attachment, including electrical and communication interfaces and mechanical mounts allowing installation of:
· power gripper,
· dexterous multi-finger hand
	

	18
	Software
	Supports ROS integration, OTA software updates, graphical programming interface, voice interaction features, and secondary development capabilities
	

	19
	Safety requirements

	Robot must include dual emergency stop (on-robot and remote), safe boot / controlled restart, and secure remote access
	

	20
	Mobility performance
	Robot must be capable of stable walking at no less than 1.0 m/s, step over obstacles of at least 10 cm, and maintain balance during dynamic tasks
	

	21
	Warranty
	No less than 12 months
	

	22
	Technical support
	Supplier must describe the provided support procedure
	

	23
	Reaction time
	All equipment malfunctions and/or defects be rectified online or real time within no more than 3 working days from the moment they are detected or upon receipt of a notification from the Contracting Authority (the time for rectification of the malfunction and/or defect is calculated from whichever of these moments occurs first).
If it is not possible to eliminate the malfunction and/or defect within 3 working days, the Supplier must replace the faulty equipment or component with a functionally equivalent one.
	

	24
	Notes
	The technical offer must clearly and unambiguously indicate any operational limitations.
(The supplier is entitled to provide information on such limitations either by describing them in this technical offer form or by attaching them as a separate annex to the technical offer.)
	

	25
	Other
	Delivery conditions (place, time, etc.): DDP-Ventspils, Latvia (Incoterms2020) to Ganību iela 99, Ventspils, LV-3601, Latvia
	

	26
	
	All equipment must be new, unused, delivered functional, ready for operation
	











	Finanšu piedāvājums/Financial offer
	EUR

	5
	The Contract Price, total
	

	including sub-positions:
The list of sub-positions may be expanded at the applicant's discretion if necessary to meet the minimum technical requirements

	5.1.
	force controlled three-fingered dexterous hand (left)
	

	5.2.
	multi-joint five-fingered dexterous hand (right)
	

	5.3.
	battery, 3 units
	

	5.4.
	remote
	

	5.5.
	protective bracket
	

	5.6.
	360 Lidar
	

	5.7.
	Depth Camera
	

	5.8.
	Dock station
	

	
	..
	

	
	Advance payment requested
(not exceeding 30% of the Contract Price, total)
	



	The quotations and prices offered must be fixed for the entire period of execution of the Procurement Agreement and must not be subject to any subsequent recalculations.

	The contracting authority has the right to refuse to conclude the agreement within the framework of the procurement, as well as to reduce or increase (from any sub-position equipment, if any is offered) the equipment by 10% of the total contract price in accordance with the items of the financial offer in sub-positions (e.g., if the tenderer offers 2 (two) units of equipment, the Customer has the right to choose to purchase 1 (one) unit of equipment), without changing the unit prices indicated in the tenderer's financial offer.

	The Contracting Authority is entitled not later than one day before the end of the specified deadline for submission of procurement proposals to make amendments to the procurement documentation, including attaching additional documents or updating the attached documents, as well as to extend the deadline for submission of procurement proposals, ensuring that the deadline for submission of procurement proposals after the relevant notice has been published on the website of the Procurement Monitoring Bureau is not shorter than five working days.

	The Contracting Authority is entitled to negotiate with suppliers.

	The Contracting Authority shall select the offer that is most economically advantageous for the Contracting Authority and best satisfies its needs, as well as ensures the effective use of the financing allocated by the contracting authority.

	[bookmark: _GoBack]By issuing this offer tenderer commits to fulfill all requirements of procurement documents.
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