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	Lot No. 9

	9.1.
	High-Performance Warehouse Reach Truck
	1
	· Battery type – Lithium-ion, not less than 300 Ah
· Battery installation – Rail-mounted
· Mast – 3-stage mast, lifting height 10000 mm or higher, with free lift; mast height in lowered position not exceeding h1 = 3950 mm
· Maximum load capacity at maximum lifting height – not less than 900 kg
· Distance between support forks – 900 ± 40 mm
· Hydraulic control
· Steering angle – 360°
· Overhead operator protective guard
· Fork length – 1150 ± 10 mm
· With side shift
· Fork tilt – 4° forward, 2° backward
· User manual in Latvian language and electronic format
· Load backrest – 1000 mm
· Charger included
· Automatic 0-position fork tilt
· Automatic 0-position side shift
· Blue LED safety light (in the direction of the drive wheel)
· Height indicator
· Fork positioning laser
· Camera system
· Armrest
· DC/DC converter 48V/12V, with outlet on the control panel
· Delivery, installation and staff training included.







