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I. GENERAL INFORMATION

1. Procurement information:
[bookmark: _Hlk211424922]1.1. The procurement is organized in accordance with the requirements set out in the Cabinet of Ministers Regulations No. 104 of February 28, 2017 [footnoteRef:2](hereinafter – Cabinet Regulations) and the regulations. [2: Available at https://likumi.lv/ta/id/289082-noteikumi-par-iepirkuma-proceduru-un-tas-piemerosanas-kartibu-pasutitaja-finansetiem-projektiem ] 

1.2. The procurement is carried out within the framework of the “Second round of project application selection for the specific support objective 1.2.1. “Strengthening research and innovation capacity and introduction of advanced technologies to enterprises” of the European Union Cohesion Policy Programme 2021–2027, measure 1.2.1.1. “Support for the development and internationalisation of new products”.
1.3. Any Applicant who complies with the requirements of these Regulations and submits a bid may participate in the Procurement.
1.4. Terms used in the Regulations.
The interested supplier is the supplier who has received the procurement documents.
A Bidder is an Interested Supplier who has submitted their bid in the procurement.
2. Procurement identification number: No. EHT 2026/03/1
3. Customer information
3.1. [bookmark: _Hlk211336758]Customer: – SIA "EcoHeat Technologies"
3.2. Registration No. 40203155061
3.3. Legal address: Langervaldes Street 2, Raubēni, Cenu parish, Jelgava county, LV-3002
3.4. Delivery address of the procurement object: Brīvības Street 103, Liepāja, LV-3401
3.5. Contact person:
[bookmark: _Hlk211340220]SIA "EcoHeat Technologies" Lawyer Jana Laporte, tel.: +37125617270 , e-mail: jana.laporte@ecoheatholdings.lv
3.6. Working hours: weekdays from 8:00-17:00.
4. Description and scope of the procurement subject
4.1. “Supply of raw materials and tools for the needs of the project of SIA “EcoHeat Technologies”” in accordance with the requirements of the procurement regulations, and the terms of the contract.
[bookmark: _Hlk211424535]The Applicant must take into account that the indicated amount is indicative and the Customer has the right to purchase both a larger and a smaller amount of the procurement item specified in the Technical Specification , as well as the Customer may purchase the procurement item in installments until December 31, 2027 .
4.2. The subject of the procurement is divided into parts.
5. Place, date, time and procedure for submitting bids
5.1. The offer must be submitted by April 10, 2026, at 12:00 , by sending the offer electronically to the e-mail address: jana.laporte@ecoheatholdings.lv .
6. Requesting and providing additional information and access to procurement documentation
6.1. Communication between the Customer and Interested Suppliers and/or Applicants within the framework of the procurement shall be in Latvian or English via e-mail.
6.2. The communication document shall include the title and identification number of the procurement.
6.3. The Applicant shall send the communication document to the e-mail address of the Client specified in the Regulations. The Applicant may also submit the communication document to the Client at the address specified in Clause 3 during working hours.
6.4. The contracting authority shall publish the procurement notice in the Publication Management System of the Procurement Monitoring Bureau, ensuring free and direct electronic access to the procurement regulations, its annexes and all additional necessary documents.
6.5 . If the customer provides additional information, it shall post this information at the address specified in clause 6.4, also indicating the question asked.
6.6. The Customer is entitled to make amendments to the procurement documentation, including adding additional documents or updating the attached documents, as well as extend the deadline for submitting tenders, in accordance with Paragraph 24 of the Cabinet of Ministers' Regulations, no later than one day before the end of the specified deadline for submitting tenders.
6.7. Applicants are obliged to familiarize themselves with the information about the procurement, which will be published at the address specified above.
7. The estimated (indicative) total contract price of the procurement subject is EUR 300,000.

II. REQUIREMENTS FOR THE PREPARATION AND SUBMISSION OF THE OFFER
8. The Applicant is entitled to submit a bid for one, several, or all Procurement items specified in Annex No. 2.
9. The offer must fully comply with the requirements set out in the regulations and their annexes.
10. The applicant must submit one proposal in electronic format.
11. The offer must be submitted in computer printout, in Latvian or English.
12. The tenderer may amend or withdraw the submitted tender before the expiry of the tender submission period.
13. All annexes to the offer are its integral parts.
14. The offer shall be signed by the Applicant's authorized signatory or an authorized person.
15. All information provided in the Applicant's offer must be true. If the Client has doubts about the truthfulness of the information provided in the Applicant's offer or the authenticity of a copy of a document, it has the right to request that the Applicant confirm the truthfulness of the information and/or present the original of a confirming document or submit a certified copy of the document.


III. REQUIREMENTS FOR THE APPLICANT, QUALIFICATION DOCUMENTS TO BE SUBMITTED BY THE APPLICANT
16. Applicant qualification requirements, documents to be submitted.
	
	Requirements
	
	Documents to be submitted

	General qualification requirements

	16.1
	The applicant has applied to participate in the procurement.
	16.1.1.
	An application letter, prepared and completed in accordance with the attached form (Annex No. 1), which must be signed by the head of the Applicant's company or an authorized representative.

	16.2.
	Applicant, is registered in the Commercial Register of the Enterprise Register of the Republic of Latvia or in an equivalent register abroad, in accordance with the procedures specified in regulatory enactments, in accordance with the requirements of the regulatory enactments of the relevant country.
	16.2.1.
	The Client will check information about companies registered in Latvia in publicly available sources and databases.
A company registered abroad must submit a copy of the commercial register or an equivalent certificate from an institution registering commercial activities, or a copy of a certificate issued by the relevant institution, or a reference to a source where the Client can verify the Applicant's compliance with the requirements of Clause 16.2.

	16 .3.
	The restrictions set out in the first part of Article 11.1 of the Law on International and National Sanctions of the Republic of Latvia do not apply to the Applicant .
	16.3.1.
	The Customer shall verify the inapplicability of this exclusion condition on websites:
1) http://sankcijas.fid.gov.lv/ 
2)
https://www.sanctionsmap.eu/#/main
3 ) https://www.treasury.gov/resource-center/sanctions/SDN-List/Pages/consolidated.aspx  




IV. REQUIREMENTS FOR THE CANDIDATE, TECHNICAL AND FINANCIAL BID DOCUMENTS TO BE SUBMITTED BY THE CANDIDATE

17. The Applicant's technical and financial offer must be prepared and submitted in accordance with the technical and financial offer template (Annex No. 2), in relation to the Procurement position in which the Applicant wishes to submit its offer.
18. If a specific manufacturer is specified in the Technical Specification, the Applicant may submit an analogous product. When offering analogues of the raw material, the Applicant must submit a variant of the offer with the declarations of conformity of the manufacturer of the analogous materials and technical documentation.
19. 	The applicant's financial proposal must be prepared in accordance with the following requirements :
19.1. The bid price must include all planned expenses necessary for the execution of the procurement contract in full and of appropriate quality in accordance with the applicable regulatory enactments. The financial bid must include all expenses that will arise during the execution of the procurement contract. Financial bid;
19.2. When evaluating the offer, the Customer will take into account the total price indicated in the offer excluding value added tax.

V. OPENING, EVALUATION AND DECISION-MAKING OF BIDDS

19. The contracting authority shall open the submitted tenders immediately after the deadline for submission of tenders.
20. The evaluation of the offers is carried out by a responsible person designated by the Client. The decision is documented, ensuring the demonstrability and transparency of the procurement process.
21. Before selecting a tender in accordance with paragraph 23 of the Regulations, the Customer has the right to negotiate in order to align its needs with the capabilities of the Suppliers and to receive the most economically advantageous tenders. During the negotiations, the Customer has the right to ask the Tenderers to explain, supplement and improve their tenders.
22. At any time until the final decision is made on the results of the procurement procedure, the Customer has the right to invite other suppliers to submit tenders, as well as to invite them to negotiations.
23. The criterion for selecting the tender is the most economically advantageous tender, which will be determined taking into account only the offered price. The Customer reserves the right to conclude a contract with two tenderers in each of the positions who have submitted the most economically advantageous tender and the next most economically advantageous tender, which is in accordance with the Procurement requirements and, respectively, with the lowest price and the second lowest price . If the Customer chooses to conclude contracts with two tenderers in one or more positions, then when purchasing a specific product within the contract period, the Customer will choose the supplier whose product has the cheapest price at the time of the request.
24. If the selected Applicant refuses to conclude a procurement contract with the Customer, the Customer shall decide to conclude a contract with the next Applicant who has submitted the most economically advantageous tender or to terminate the procurement without selecting any tender.
25. The Customer has the right not to select any offer if the Applicants' offers do not meet the Customer's financial capabilities.
26. The Client shall, within 5 working days, simultaneously (on the same day) inform all Applicants of the decision to award the contract by sending the information electronically.
27. The Client undertakes that the processing and storage of the obtained personal data will be ensured in accordance with the requirements of Regulation (EU) 2016/679 of the European Parliament and of the Council of 27 April 2016 on the protection of natural persons with regard to the processing of personal data and on the free movement of such data, and repealing Directive 95/46/EC, other regulatory enactments and the terms of the contract/general agreement.
28. Personal data may be disclosed to the public in accordance with the regulations of the Cabinet of Ministers and the scope of legal acts issued on their basis.
29. The Customer has the right to obtain and verify the data of natural persons involved in the implementation of the procurement in public registers in accordance with regulatory enactments and to the extent specified in regulatory enactments.
30. The following annexes are attached as an integral part of the procurement:
1. Annex – Application (form);
2. Annex – Technical and Financial Proposal (form).

Appendix No. 1
[bookmark: _Hlk529455419][bookmark: _Hlk33815153]"Supply of raw materials and tools
"EcoHeat Technologies" Ltd. for project purposes"
Procurement identification No. EHT 2026/03/1
bylaws


PIETEIKUMSPARTICIPATION IN THE PROCUREMENT


	1.
	Name:

	2.
	Reg.No.

	3.
	Taxpayer registration number:

	4.
	Registration place:

	5.
	Registration year:

	6.
	Legal address:

	7.
	Office address:
Phone:
Email:

	8.
	Bank:

	9.
	Bank code:

	10.
	Account No.:

	12.
	Contact person:


1. [bookmark: _Hlk213139597]Having familiarized ourselves with the regulations of the procurement organized by the Customer “Supply of raw materials and tools for the needs of the project of SIA “EcoHeat Technologies”” Procurement Identification No. EHT 2026/03/1 (hereinafter – Nolikums), accepting all the requirements set out in the Regulations,
we submit a proposal consisting of this application and the Technical and Financial Proposal (hereinafter referred to as the Proposal),

2. We offer to make the deliveries specified in the procurement “Supply of raw materials and tools for the needs of the project of SIA “EcoHeat Technologies”” Procurement identification No. EHT 2026/03/1 in accordance with the conditions specified in the regulations and in accordance with the offer submitted in Annex 2 to the Regulations. 

3. We confirm that all information contained in the offer is true.
	



Applicant/Applicant's authorized person:

	
	
	
	
	

	/position/
	
	/signature/
	
	/first name, last name/

	
	
	
	
	

	
	
	2026 ___._______________
	
	

	/place of compilation/
	
	
	
	




[image: ]





Appendix No. 2
"Supply of raw materials and tools
"EcoHeat Technologies" Ltd. for project purposes"
Procurement identification No. EHT 2026/03/1
bylaws


	TECHNICAL AND FINANCIAL OFFER






	No.
	Name
	Chemical composition / description
	Standard/Specification
	Indicative volume
	Cost per unit

	1
	Alloying additives and ferroalloys
	
	
	
	

	1.1
	Carburetor RANCO (synthetic graphite)
	C 95–99+; ash ≤2–5; S ≤0.01–0.03; low N
	According to manufacturer's specifications
	62.5 kg
	

	1.2
	Nickel metal (Class I)
	Ni ≥99.8; impurities — according to COA
	LME Class I / ASTM
	162.5 kg
	

	1.3
	Ferromanganese LC
	Mn 65–78; Fe balance; C ≤0.5; Si ≤1.5; P ≤0.3; S ≤0.03
	ISO 5446:2017
	415 kg
	

	1.4
	Ferromanganese MC
	Mn 72–78; Fe balance; C 1.0–2.0; Si ≤2.0; P ≤0.3; S ≤0.03
	ISO 5446:2017
	177.5 kg
	

	1.5
	Ferrosilicon FeSi75
	Si 74–78; Fe balance; Al ≤2.0; C ≤0.5; P ≤0.05; S ≤0.02
	ISO 5445
	110 kg
	

	1.6
	Ferrochrome LC (≈65% Cr)
	Cr 60–70; Fe balance; C ≤0.06; Si ≤2.0; P ≤0.05; S ≤0.03
	ISO 5448
	182.5 kg
	

	1.7
	Ferromolybdenum FeMo60
	Mo 60–70; Fe balance; C ≤0.1; Si ≤1.0; P ≤0.05; S ≤0.05; Cu ≤0.5
	ISO 5452
	60 kg
	

	1.8
	Ferrovanadium FeV80 LC
	V 75–85; Fe balance; C ≤0.25; Si ≤1.5; Al ≤2.0; P ≤0.05; S ≤0.05
	ISO 5451:2022
	3.5 kg
	

	1.9
	Ferrotitanium FeTi70 LC
	Ti 65–75; Fe balance; Al 1.5–6.0; Si ≤4.0; C ≤0.2; P ≤0.05; S ≤0.05
	ISO 5454:1980
	10 kg
	

	1.10
	Calcium silicon CaSi30
	Ca 28-32; Si 58-62; Al ≤1.5; C ≤1.0; P ≤0.05; S ≤0.05
	According to manufacturer's specifications
	50 kg
	

	1.11
	Mismetal (Ce–La–Nd)
	Ce 45–55; La 20-35; Nd 10-15; Pr 3-5
	According to manufacturer's specifications
	50 kg
	

	2
	Refractory materials (linings)
	
	
	
	

	2.1
	Silicomix (acid lining)
	SiO₂ base, binder B₂O₃ ≈ 0.6%
	Capital Refractories
	1000 kg
	

	2.2
	Spinel-forming lining
	Spinel-forming mass based on Al₂O₃–MgO
	Capital Refractories
	1000 kg
	

	2.3
	Capram 70 or analog (plastic fireproof lining) mass for the repair and lining of casting ladles and furnaces).
	Collar/repair mass, also suitable for ladle lining
	Capital Refractories
	1000 kg
	

	3
	Moulding and auxiliary materials
	
	
	
	

	3.1
	Quartz sand
	Washed, dried, fractionated
	EN/ISO
	2 tons
	

	3.2
	Resin (for Alphaset process)
	Alkaline phenolic resin (Alphaset, ester-cured no-bake system)
	According to manufacturer's specifications
	100 kg
	

	3.3
	Hardener (for Alphaset process)
	Ester hardener for alkaline phenolic resins
	According to manufacturer's specifications
	20 kg
	

	3.4
	Coating, zircon-based
	Based on ZrSiO₄
	According to manufacturer's specifications
	10 kg
	

	3.5
	Coating, magnesite-based
	MgO-based
	According to manufacturer's specifications
	10 kg
	

	4
	Equipment and tools
	
	
	
	

	4.1
	Thermocouples + transmitters
	10 thermocouples + 2 transmitters; external unit, immersion sensor; Tmax 1300 °C
	EN/ISO
	Set
	

	
	
	
	TOTAL:
(price excluding VAT)
	
	








	<Job title, first name and surname of the authorized signatory>

	Signature of authorized signatory>
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